**Station:** KBTF-CD

**Facility ID:** 34438

**License File #:** BLDTA20100921ABW

**Channel:** 31

**Subject:** Transmitter Power Output – Original Application

**Explanation:**

In the station’s Application for License, file number BLDTA-20100921ABW, the transmitter power output (TPO) was erroneously specified as 0.87 kW.  The -3.7 dBk value specified for the TPO is correct.  The TPO in kW should be 0.43.