MEDIA BUREAU

Video Division

 Displacement Digital Low Power TV Application Worksheet

File: 0000053789 Call: NEW

Check means everything from that line has been considered and completed when required.

X Qualifies as displacement. If already channel 36 or below must qualify.

X Licensed and Silent for less than a year.

X Cannot have other active digital channel for the same station.

X Cannot have channel 36 and above.

X Contour overlap. (CH 14-69) ext. 74dBu F(50,50) & pro. 51dBu F(50,90)

 (CH 2-6) ext. 62 dBu F(50,50) & pro. 43 dBu F(50,90)

 (CH 7-13) ext. 68 dBU F(50,50) & pro. 48 dBu F(50,90)

X Within 30 miles of license.

 X IX to pending NTSC or DTV application is OK.

X IX to existing station per LONGLEY-RICE study, letter is required.(CDBS BLOCK CODE)

X Maximum ERP not exceeded. (3 kW/VHF 15 kW/UHF)

X ASRN correct or letter required.(CDBS BLOCK CODE)

X GRANT referral letters (Can,Mex,etc) required.(CDBS BLOCK CODE)

X DA major lobes were entered.

X CALL ran and printed.(Channel changes for majors require a new call sign)

X Same expiration date as the requested CP.

X All conditions added to authorization (258).

 X Authorizations sent.

Comments:

Reviewed by: MFC Date: 06/19/18 version 9//08